0 1 2 3 4 5 6 7 8 9 10 0

0.1

0.2

0.3

0.4

0.5

0.6

0.7

0.8

0.9

1 A test of code accuracy (a narrow line at 6.4keV,..., a/M=0.4)

Energy [keV]

Radiation flux normalized to maximum

range of radii (units ofGM/c^2): 6<r<10

observer inclination:θ_0= 65^o

Factor #1: Resolution of data tables: High (model 01, tables coverr<50) Low (model 02, tables coverr<100)

Factor #2: Resolution of the code (ky_main.f; computing the predicted spectrum using data tables):

High(n_r x n_ϕ=100 x 360) - thick line Low(n_r x n_ϕ=50 x 60) - thin line